

Can I export STL files from CEREC Chairside Software?

**To Export STL Files:**

Set up a case in CEREC, Sirona Connect or Ortho Software. Capture the images, and advance to the point where the buccal bite is articulated in the Model Phase.

Click the arrow in the upper left corner of the screen. | Select Export.

Highlight the location where you want to save the file on the left hand side of the windows screen.

Use the drop down menu in the 'Save as Type' field and select .STL from the list.

 a. The user can rename the file by typing whatever they choose in the File Name field. This is optional.

Click Save.

The file is now saved in the location as directed by the user and can be copied to a flash drive or uploaded to a file sharing service as needed.

**Items to Note:**

The Open Scan Export License is free for CEREC Club members upon request.

Users must install CEREC/Sirona Connect 4.5 or Ortho 1.2 prior to requesting the license.

To request the Open Scan Export License, CEREC Club customers (or their branch representative) can call the Patterson CAD/CAM Team at 1.800.475.5036.

The license will be distributed through the sironaupdates.com portal.

Non-club customers can contact their local Patterson representative to inquire about pricing and order the license.

The Open Scan Export file type is intended for use with model printing. Users may determine if the file type is suitable for use in other formats.

For best results, it is recommended that CEREC files be scanned, designed and produced within the CEREC system.

The export of restoration design data is exclusive to inLab software with the purchase of a separate export license.